Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring an MPLS Pseudowire with VCC Cell Relay Encapsulation and Monitoring ATM Subinterfaces for Layer 2 Services over MPLS in the JunosE BGP and MPLS Configuration Guide

# show atm subinterface

#### Syntax

show atm subinterface
[ summary | atm interfaceSpecifier | summary atm interfaceSpecifier |
status operatingStatus ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays the current state of all ATM subinterfaces that you specify.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- summary—Specifies that summary information is displayed
- status—Displays information only for the ATM subinterfaces with the specified operating status
- operatingStatus—One of the following operating states:
  - dormant
  - dormantLockout
  - down
  - lowerLayerDown
  - notPresent
  - up
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Configuring an MPLS Pseudowire with VCC Cell Relay Encapsulation and Monitoring ATM Subinterfaces for Layer 2 Services over MPLS in the JunosE BGP and MPLS Configuration Guide

#### Published: 2010-07-14

Help
|
My Account
|
Log Out