Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring the HTTP Server to Support Guided Entrance in the JunosE Broadband Access Configuration Guide

# ipv6 http redirectUrl

#### Syntax

ipv6 http redirectUrl url

no ipv6 http redirectUrl

#### Release Information

Command introduced in JunosE Release 10.1.0.

Profile Configuration mode added in JunosE Release 11.0.0.

#### Description

Specifies the URL to which a subscriber's initial Web browser session is redirected, enabling initial provisioning and service selection for the subscriber. The no version removes the redirection action.

#### Options

- url—Name of the URL; 64 characters maximum

#### Mode

Interface Configuration, Subinterface Configuration, Profile Configuration

#### Related Topics

- Configuring the HTTP Server to Support Guided Entrance in the JunosE Broadband Access Configuration Guide

#### Published: 2010-07-19

Help
|
My Account
|
Log Out