Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Hierarchical QoS Parameters Overview
- Configuring a Basic Parameter Definition for QoS Administrators
- Configuring a Parameter Definition for IP Multicast Bandwidth Adjustment
- Example: QoS Parameter Configuration for Hierarchical Parameters
- qos-parameter-define

# Configuring a Parameter Definition to Calculate Hierarchical Instances

You can configure hierarchical parameters for applications where you want the system to add instances associated with child interfaces and associate the sum with a parent interface.

Hierarchical parameters have explicit instances that are associated with the logical interfaces of instance-interface types, as well as implicit instances that are associated with the logical interfaces of controlled-interface types. The system computes the values of an implicit instance as the sum of the values of the explicit instances stacked above the implicit instance.

To configure a hierarchical QoS parameter definition:

- Include the hierarchical keyword with the qos-parameter-define command.
  host1(config)#qos-parameter-define max-subscriber-bandwidth host1(config-qos-parameter-define)#

#### Related Topics

- Hierarchical QoS Parameters Overview
- Configuring a Basic Parameter Definition for QoS Administrators
- Configuring a Parameter Definition for IP Multicast Bandwidth Adjustment
- Example: QoS Parameter Configuration for Hierarchical Parameters
- qos-parameter-define

#### Published: 2010-06-30

Help
|
My Account
|
Log Out