# Stateful SRP Switchover Platform Considerations

Stateful SRP switchover is supported on all E Series routers except for the ERX310 Broadband Services Router.

For information about the modules supported on E Series routers:

- See the ERX Module Guide for modules supported on ERX7xx models and ERX14xx models.
- See the E120 and E320 Module Guide for modules supported on the E120 and E320 Broadband Services Routers.

## Module Requirements

The following table lists which SRPs support or do not support the high availability mode (stateful SRP switchover) feature.

SRP Model | Supported
--- | ---
SRP-5G | No
SRP-5G+ | Yes
SRP-10G | Yes
SRP-40G | No
SRP-40G PLUS | Yes
SRP-100 | Yes

| Note: Stateful SRP switchover requires two SRP modules with 1 GB of memory or more.

#### Related Topics

- Monitoring the Redundancy Status
- Monitoring the Redundancy Status of SRP Modules
- show redundancy
- show redundancy srp