Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# remote-neighbor

#### Syntax

For OSPF:

[ no ] remote-neighbor ipAddress area { areaId | areaIdInt }

For PIM:

[ no ] remote-neighbor [ ipAddress | ipv6Address ] sparse-mode

For RIP:

[ no ] remote-neighbor ipAddress

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an OSPF, PIM, or RIP remote neighbor. The no version removes the remote neighbor and any attributes configured for the neighbor.

| Note: For PIM, this command is typically used when you configure PIM remote neighbors to run multicast services over BGP/MPLS VPNs. That functionality is no longer supported.

#### Options

- ipAddress—IPv4 address identifying the remote neighbor
- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value, in the range 0–4294967295
- ipv6Address—IPv6 address identifying the remote neighbor

#### Mode

Router Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out