Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# nas-port-type ethernet

#### Syntax

nas-port-type ethernet { cable | wireless-80211 | wireless-cdma | wireless-umts |
wireless-1x-ev | wireless-other | iapp | value }

no nas-port-type ethernet

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the RADIUS NAS-Port-Type attribute (61) used for Ethernet interfaces. The no version removes the NAS-Port-Type setting.

#### Options

- cable—Cable
- wireless-80211—Wireless 802.11
- wireless-cdma—Wireless code division multiple access (CDMA)
- wireless-umts—Wireless universal mobile telecommunications system (UMTS)
- wireless-1x-ev—Wireless 1xEV
- wireless-other—Wireless other
- iapp—Inter Access Point Protocol (IAPP)
- value—Number in the range 0–65535

#### Mode

AAA Profile Configuration

#### Published: 2010-07-13

Help
|
My Account
|
Log Out