Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Monitoring the Policy Configuration of IPv6 Interfaces

# show ipv6 interface

#### Syntax

show ipv6 interface [ vrf vrfName ] [ brief | detail ]
[ interfaceType interfaceSpecifier ][ delta ] [ filter ]

To display summary information:

show ipv6 interface summary [ vrf vrfName ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
vrf keyword and vrfName variable added in JunosE Release 7.2.0.

#### Description

Displays current state of all IPv6 interfaces or the IPv6 interfaces that you specify. The default is all interface types and all interfaces.

#### Options

- vrfName—Name of the VRF
- brief—Displays a brief summary of IPv6 status and configuration information
- detail—Shows a detailed display of IP status and configuration information
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- delta—Displays baselined statistics
- filter—See Filtering show Commands
- summary—Shows a detailed summary of IP status and configuration

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring the Policy Configuration of IPv6 Interfaces

#### Published: 2010-07-14

Help
|
My Account
|
Log Out