Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# member-interface

#### Syntax

[ no ] member-interface interfaceType interfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Adds a member interface, also known as a bundle member, to an MLPPP bundle, an MLFR bundle, or an IEEE 802.3ad link aggregation group (LAG) bundle. The no version removes the specified member interface from the bundle.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - serial (MLFR bundle or MLPPP bundle)
  - pos (MLFR bundle only)
  - fastEthernet (IEEE 802.3ad LAG bundle only)
  - gigabitEthernet (IEEE 802.3ad LAG bundle only)
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Interface Configuration, Subinterface Configuration

#### Published: 2010-07-19

Help
|
My Account
|
Log Out