Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# timeout

#### Syntax

RADIUS:

timeout waitTime

no timeout

RTR:

timeout timeoutValue

no timeout

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

When used from RADIUS Configuration mode, specifies the interval, in seconds, before the router retransmits a RADIUS packet to an authentication or accounting server. The no version restores the default.

When used from RTR Configuration mode, specifies the timeout for a Response Time Reporter operation. The no version returns the operation to the default value. You can apply this parameter only to echo entries.

#### Options

- waitTime—Number of seconds in the range 1–1000; default value is 3
- timeoutValue—Number in milliseconds that the operation waits for a response; if the value is set to 0 or is larger than frequency, it will be ignored; default value is 5000

#### Mode

RADIUS Configuration, RTR Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out