# mode

#### Syntax

mode { file-system-synchronization | high-availability }

no mode

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables high availability mode (hitless SRP switchover) operation. The no version returns high availability mode operation to its default (file-system-synchronization).

#### Options

- file-system-synchronization—Uses file synchronization to keep the configuration of the standby SRP coordinated with the configuration of the active SRP
- high-availability—Uses mirroring to keep the configuration and state of the standby SRP coordinated with the configuration and state of the active SRP

#### Mode

Redundancy Configuration