Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# ip vrrp virtual-address

#### Syntax

ip vrrp vrid virtual-address { auto | ipAddress ipAddress [ ipAddress ipAddress ]* }

no ip vrrp vrid virtual-address [ ipAddress ipAddress ]*

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Associates an IP address with a VRID. The no version removes a list of IP addresses associated with a VRID. The no version clears the auto flag, if auto addresses are being used. There is no default.

#### Options

- vrid—VRID identifier; a number in the range 1–255
- auto—Automatically learns or configures associated addresses depending on the priority.
- ipAddress—IP address
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Interface Configuration

#### Published: 2010-07-19

Help
|
My Account
|
Log Out