Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# show subscribers

#### Syntax

To display detailed information:

show subscribers [ ipv6 [ ipv6Prefix ] ]
[ domain domainName | icr-partition icrPartitionLocationId |
interface { atm | ethernet | lag } interfaceSpecifier |
port interfaceSpecifier | slot slotNumber | username userName |
virtual-router vrName ] [ filter ]

To display summary information:

show subscribers summary [ domain | icr-partition | interface | port | slot | virtual-router ]
[ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
interface, atm, and ethernet keywords added in JunosE Release 7.3.0.
slot keyword and slotNumber variable added in JunosE Release 7.3.0.
icr-partition keyword and icrPartitionLocationId variable added in JunosE Release 10.3.0.
lag keyword added in JunosE Release 11.0.0.

#### Description

Displays the active subscribers on your router.

#### Options

- ipv6—Displays IPv6 subscribers for the domain
- ipv6Prefix—Prefix that defines the IPv6 network that you want to filter
- userName—Username of active subscriber
- domain—Displays active subscribers for the domain
- domainName—Domain name matching usernames of active subscribers
- icr-partition—Displays active subscribers for the ICR partition
- icrPartitionLocationId—A unique identifier for each ICR partition on a chassis. Note that this ID different from the partition ID, which is configured using the ip vrrp vrid icr-partition partitionId command. The partition location ID that you specify here is a combination of the interface within the chassis on which the ICR partition is configured and the VRRP ID, which is system-defined and nonconfigurable.
- interface—Displays active subscribers for the specified interface: atm, ethernet, or lag. In the summary version, displays active subscribers for all ATM, Ethernet, and LAG interfaces
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- port—Displays active subscribers for the port
- slot—Displays active subscribers for the slot
- slotNumber—Number of the chassis slot of the line module in the range 0–2 (ERX310 model), 0–6 (ERX7xx models), 0–13 (ERX14xx models), 0-5 (E120 router), and 0-16 (E320 router)
- virtual-router—Displays active subscribers for the VR
- vrName—Name of the VR to which interfaces of active subscribers are bound
- filter—See Filtering show Commands
- summary—Displays the active subscribers for each domain, interface, port, slot, or virtual router

#### Mode

Privileged Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out