[ Contents] [ Prev] [ Next] [ Report an Error]

# FE-2 Module Combination (2 Ports)

> Line module label | FE-2
> I/O module label | FE-2 I/O
> Number of I/O ports | 2
> Software release | First supported: 1.3.0 Last supported: 7.0.x
> Description | 60 W Fast Ethernet
> Type | Non-ASIC
> Capability | IEEE 802.3 standards compliance 10/100Base-T
> Software features | See ERX Module Guide, Appendix A, Module Protocol Support for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | ERX-7xx models ERX-1410 router
> SRP module compatibility | SRP-5G SRP-5G+ SRP-10G
> Module redundancy support | Not applicable
> Cables and connectors | Accepts up to two RJ-45 connectors. For 10-Mbps operation, use CAT 3, 4, or 5 UTP cable. For 100-Mbps operation, use only CAT 5 UTP cable. The transmitted signal complies with IEEE 802.3/802.3u for cable lengths up to 100 m (328 feet). See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See ERX Module Guide, Appendix B, Module LEDs.
> Alarms, errors, and events | See Monitoring Ethernet Interfaces in the Configuring Ethernet Interfaces chapter of the JUNOSe Physical Layer Configuration Guide for Release 8.0.x and earlier.

[ Contents] [ Prev] [ Next] [ Report an Error]