# rtr

#### Syntax

[ no ] rtr rtrIndex

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the number of the RTR operation to be configured and accesses the RTR Configuration mode. The no version removes all configuration information for a specified RTR operation.

| Note: The no rtr has a different function than the no rtr rtrIndex command.

#### Options

- rtrIndex—Number of the operation to be configured, in the range 1–4294967295; there is no default

#### Mode

Global Configuration

#### Related Topics

- no rtr command