Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# ip initial-sequence-preference

#### Syntax

ip initial-sequence-preference preference

no ip initial-sequence-preference

#### Release Information

Command introduced in JunosE Release 8.1.0.

#### Description

Configures the warm restart replay preference for an IP interface after a high availability switchover. The no version restores the default value.

#### Options

- preference—Preference value, 0 or 1; 1 indicates highest preference; default value is 0

#### Mode

Subinterface Configuration

#### Published: 2010-07-19

Help
|
My Account
|
Log Out