Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring Tunnel Subscriber Authentication in the JunosE Broadband Access Configuration Guide

# tunnel-subscriber authentication

#### Syntax

tunnel-subscriber authentication { enable | disable }

no tunnel-subscriber authentication

#### Release Information

Command introduced in JunosE Release 9.1.0.

#### Description

Configures whether tunnel subscribers within the domain map are authenticated with the authentication server or are granted access without individual authentication. The no version restores the default condition, where users are not authenticated by an authentication server.

#### Options

- enable—Enables tunnel subscriber authentication by the authentication server
- disable—Disables tunnel subscriber authentication by the authentication server; all users in the domain are granted access without individual authentication; this is the default condition

#### Mode

Domain Map Configuration

#### Related Topics

- Configuring Tunnel Subscriber Authentication in the JunosE Broadband Access Configuration Guide

#### Published: 2010-07-14

Help
|
My Account
|
Log Out