Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- To identify the type of ASIC used by a line module, see the ERX Module Guide and the E120 and E320 Module Guide
- Guidelines for Managing Queue Thresholds
- Guidelines for Managing Buffers

# Memory Requirements for Queue and Buffers

JunosE Software uses 128-byte buffers.

The egress memory available for queues available depends on the ASIC and the line module. Table 1 lists the egress memory.

Table 1: Egress Memory and Region Size on ASIC Line Modules

ASIC | Line Module | Egress Memory (MB) | Region Size (MB)
--- | --- | --- | ---
EFA | All EFA line modules | 32 | 4
FFA | GE-2 and GE-HDE | 64 | 8
| OC48 | 128 | 16
ES2 4G LM | 128 | 16
TFA | ES2 10G LM | 96 | 12

#### Related Topics

- To identify the type of ASIC used by a line module, see the ERX Module Guide and the E120 and E320 Module Guide
- Guidelines for Managing Queue Thresholds
- Guidelines for Managing Buffers

#### Published: 2010-06-30

Help
|
My Account
|
Log Out