Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# show bgp ipv6 next-hops

#### Syntax

show bgp ipv6
[ unicast | multicast | vpnv6 all | vpnv6 vrf vrfName | route-target signaling ]
next-hops [ ipv6Address ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
route-target signaling keywords added in JunosE Release 8.2.0.

#### Description

Displays information about IPv6 BGP next hops.

#### Options

- unicast—Specifies the IPv6 unicast address family and routing table; the default option
- multicast—Specifies the IPv6 multicast address family and routing table
- vpnv6 all—Specifies the VPN-IPv6 address family and all IPv6 VPN routing and forwarding instances
- vpn6 vrf vrfName—Specifies the VPN-IPv6 address family and only the IPv6 VPN routing and forwarding instance with the name vrfName
- route-target signaling—Specifies the route-target address family
- ipv6Address—Information only for this indirect next hop
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out