# Merging Policies Configuration

In the following example IP policy p1 and IP policy p2 are attached at interface atm5/0.1 as input attachments. Subsequently, policy p3 is attached at the same point. Then policies p1 and p2 are attached as output at atm 5/0.2.

1. Create IP policy p1.
   host1(config)#ip classifier-list C1 tcp host 1.1.1.1 any eq 80 host1(config)#ip classifier-list C2 icmp any any 8 0 host1(config)#ip policy-list p1 host1(config-policy)#classifier-group C1 precedence 90 host1(config-policy-classifier-group)#forward next-hop 10.1.1.1 host1(config-policy-classifier-group)#exit host1(config-policy)#classifier-group C2 precedence 10 host1(config-policy-classifier-group)#filter host1(config-policy-classifier-group)#exit
2. Create IP policy p2.
   host1(config)#ip classifier-list C1 tcp host 1.1.1.1 any eq 80 host1(config)#ip classifier-list C3 ip any host 2.2.2.2 host1(config)#ip policy-list p2 host1(config-policy)#classifier-group C1 precedence 90 host1(config-policy-classifier-group)#forward next-hop 20.1.1.1 host1(config-policy-classifier-group)#exit host1(config-policy)#classifier-group C3 precedence 10 host1(config-policy-classifier-group)#filter host1(config-policy-classifier-group)#exit host1(config-policy)#classifier-group * precedence 1000 host1(config-policy-classifier-group)#forward host1(config-policy-classifier-group)#exit
3. Attach IP policy p1 as input at interface atm5/0.1.
   host1(config)#Interface atm 5/0.1 host1(config-subif)#ip policy input p1 statistics enable merge host1(config-subif)#exit
4. Attach IP policy p2 as input at interface atm 5/0.1. A merged policy is created.
   host1(config)#Interface atm 5/0.1 host1(config-subif)#ip policy input p2 statistics enable merge host1(config-subif)#exit
5. Display the policy lists.

       host1#show policy-list

                                         Policy Table
                                         ------ -----
       IP Policy p1
          Administrative state: enable
          Reference count:      1
          Classifier control list: C2, precedence 10
             filter
          Classifier control list: C1, precedence 90
             forward
                Virtual-router: default
                List:
                  next-hop 10.1.1.1, order 100, rule 2 (active)

          Referenced by interfaces:
             None

          Referenced by profiles:
             None

          Referenced by merge policies:
             mpl_5

       IP Policy p2
          Administrative state: enable
          Reference count:      1
          Classifier control list: C3, precedence 10
             filter
          Classifier control list: C1, precedence 90
             forward
                Virtual-router: default
                List:
                  next-hop 20.1.1.1, order 100, rule 3 (active)
          Classifier control list: *, precedence 1000
             forward

          Referenced by interfaces:
             None

          Referenced by profiles:
             None

          Referenced by merge policies:
             mpl_5

       IP Policy mpl_5
          Administrative state: enable
          Reference count:      1
          Classifier control list: C2, precedence 10
             filter
          Classifier control list: C3, precedence 10
             filter
          Classifier control list: C1, precedence 90
             forward
                Virtual-router: default
                List:
                  next-hop 10.1.1.1, order 100, rule 2 (active)
                  next-hop 20.1.1.1, order 100, rule 3 (reachable)
          Classifier control list: *, precedence 1000
             forward

          Referenced by interfaces:
             ATM5/0.1  input policy, statistics enabled, virtual-router default

          Referenced by profiles:
             None

          Component policies:
             p1
             p2

6. Show configuration.

       host1#show conf

       ! Configuration script being generated on TUE APR 26 2005 17:33:01 UTC
       ! Juniper Edge Routing Switch ERX1440
       ! Version: 9.9.9 development-4.0 (April 4, 2005  15:39)
       ! Copyright (c) 1999-2005 Juniper Networks, Inc.  All rights reserved.
       !
       ! Commands displayed are limited to those available at privilege level 15
       !
       …
       interface atm 5/0.1
        ip policy input p1 statistics enabled merge
        ip policy input p2 statistics enabled merge
        exit
       …
       …
       ip policy-list p1
        classifier-group C2 precedence 10
         filter
        classifier-group C1 precedence 90
         forward next-hop 10.1.1.1
       !
       ip policy-list p2
        classifier-group C3 precedence 10
         filter
        classifier-group C1 precedence 90
         forward next-hop 20.1.1.1
        classifier-group * precedence 1000
         forward
       !
       …
       …
       ! End of generated configuration script.

7. Display interface statistics.

       host1#show ip interface atm 5/0.1

       ATM5/0.1 line protocol Atm1483 is up, ip is up
         Network Protocols: IP
         Internet address is 99.99.99.2/255.255.255.0
         Broadcast address is 255.255.255.255
         Operational MTU = 9180  Administrative MTU = 0
         Operational speed = 155520000  Administrative speed = 0
         Discontinuity Time = 721112
         Router advertisement = disabled
         Proxy Arp = disabled
         Network Address Translation is disabled
         TCP MSS Adjustment = disabled
         Administrative debounce-time = disabled
         Operational debounce-time    = disabled
         Access routing = disabled
         Multipath mode = hashed
         Auto Configure = disabled
         Auto Detect = disabled
         Inactivity Timer = disabled

         In Received Packets 0, Bytes 0
           Unicast Packets 0, Bytes 0
           Multicast Packets 0, Bytes 0
         In Policed Packets 0, Bytes 0
         In Error Packets 0
         In Invalid Source Address Packets 0
         In Discarded Packets 0
         Out Forwarded Packets 0, Bytes 0
           Unicast Packets 0, Bytes 0
           Multicast Routed Packets 0, Bytes 0
         Out Scheduler Dropped Packets 0, Bytes 0
         Out Policed Packets 0, Bytes 0
         Out Discarded Packets 0

         IP policy input mpl_5
           classifier-group C2 entry 1
             0 packets, 0 bytes
             filter
           classifier-group C3 entry 1
             0 packets, 0 bytes
             filter
           classifier-group C1 entry 1
             0 packets, 0 bytes
             forward
           classifier-group *
             0 packets, 0 bytes
             forward
         queue 0: traffic class best-effort, bound to ip ATM5/0.1
           Queue length 0 bytes
           Forwarded packets 0, bytes 0
           Dropped committed packets 0, bytes 0
           Dropped conformed packets 0, bytes 0
           Dropped exceeded packets 0, bytes 0

8. Attach IP policy p1 at atm 5/0.2 as output.
   host1(config)#interface atm 5/0.2 host1(config-subif)#ip policy output p1 statistics enable merge host1(config-subif)#exit
9. Attach IP policy p2 at atm 5/0.2 as output. Merge policy mpl_5 is now attached.
   host1(config)#interface atm 5/0.2 host1(config-subif)#ip policy output p2 merge host1(config-subif)#exit
10. Display policies to verify that mpl_5 is created.

        host1#show policy-list

                                          Policy Table
                                          ------ -----
        IP Policy p1
           Administrative state: enable
           Reference count:      1
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_5

        IP Policy p2
           Administrative state: enable
           Reference count:      1
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 20.1.1.1, order 100, rule 3 (active)
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_5

        IP Policy mpl_5
           Administrative state: enable
           Reference count:      2
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)
                   next-hop 20.1.1.1, order 100, rule 3 (reachable)
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              ATM5/0.1  input policy, statistics enabled, virtual-router default
              ATM5/0.2  output policy, statistics enabled, virtual-router default

           Referenced by profiles:
              None

           Component policies:
              p1
              p2

11. Create and attach IP policy p3 at atm 5/0.1. A new merge policy mpl_7 is created, which is a combination of p1, p2, and p3. The previous merge policy attachment is removed.
    host1(config)#ip classifier-list C4 udp host 1.1.1.1 any eq 900 host1(config)#ip policy-list p3 host1(config-policy)#classifier-group C4 precedence 900 host1(config-policy-classifier-group)#color red host1(config-policy-classifier-group)#exit host1(config-policy)#classifier-group C1 precedence 80 host1(config-policy-classifier-group)#color yellow host1(config-policy-classifier-group)#exit host1(config-policy)#exit host1(config)#interface atm 5/0.1 host1(config-subif)#ip policy input p3 statistics enable merge host1(config-subif)#exit
12. Display policies to verify that mpl_5 and mpl_7 have been created.

        host1#show policy-list

                                          Policy Table
                                          ------ -----
        IP Policy p1
           Administrative state: enable
           Reference count:      2
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_5
              mpl_7

        IP Policy p2
           Administrative state: enable
           Reference count:      2
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 20.1.1.1, order 100, rule 3 (active)
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_5
              mpl_7

        IP Policy p3
           Administrative state: enable
           Reference count:      1
           Classifier control list: C1, precedence 80
              color yellow
           Classifier control list: C4, precedence 900
              color red

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_7

        IP Policy mpl_5
           Administrative state: enable
           Reference count:      1
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)
                   next-hop 20.1.1.1, order 100, rule 3 (reachable)
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              ATM5/0.2  output policy, statistics enabled, virtual-router default

           Referenced by profiles:
              None

           Component policies:
              p1
              p2

        IP Policy mpl_7
           Administrative state: enable
           Reference count:      1
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 80
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)
                   next-hop 20.1.1.1, order 100, rule 3 (reachable)
              color yellow
           Classifier control list: C4, precedence 900
              color red
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              ATM5/0.1  input policy, statistics enabled, virtual-router default

           Referenced by profiles:
              None

           Component policies:
              p1
              p2
              p3

13. Detach p2 from atm 5/0.1. A new merge policy mpl_8 is created, which is a combination of p1 and p3. The previous merge policy mpl_7 is detached and, because this policy has no attachments, it is deleted.
    host1(config)#interface atm 5/0.1 host1(config-subif)#no ip policy input p2 host1(config-subif)#exit
14. Display policies to verify that the mpl_7 is removed and the new merge policy mpl_8 is created.

        host1#show policy-list

                                          Policy Table
                                          ------ -----
        IP Policy p1
           Administrative state: enable
           Reference count:      2
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_5
              mpl_8

        IP Policy p2
           Administrative state: enable
           Reference count:      1
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 20.1.1.1, order 100, rule 3 (active)
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_5

        IP Policy p3
           Administrative state: enable
           Reference count:      1
           Classifier control list: C1, precedence 80
              color yellow
           Classifier control list: C4, precedence 900
              color red

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_8

        IP Policy mpl_5
           Administrative state: enable
           Reference count:      1
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)
                   next-hop 20.1.1.1, order 100, rule 3 (reachable)
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              ATM5/0.2  output policy, statistics enabled, virtual-router default

           Referenced by profiles:
              None

           Component policies:
              p1
              p2

        IP Policy mpl_8
           Administrative state: enable
           Reference count:      1
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C1, precedence 80
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)
                   next-hop 20.1.1.1, order 100, rule 3 (reachable)
              color yellow
           Classifier control list: C4, precedence 900
              color red

           Referenced by interfaces:
              ATM5/0.1  input policy, statistics enabled, virtual-router default

           Referenced by profiles:
              None

           Component policies:
              p1
              p3

15. Detach p1 from atm 5/0.1. Merge policy mpl_8 is detached and deleted, and only p3 is attached to this interface.
    host1(config)#interface atm 5/0.1 host1(config-subif)#no ip policy input p1 host1(config-subif)#exit
16. Display policies to verify that p3 is attached to atm 5/0.1 and mpl_8 is removed.

        host1#show policy-list

                                          Policy Table
                                          ------ -----
        IP Policy p1
           Administrative state: enable
           Reference count:      1
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_5

        IP Policy p2
           Administrative state: enable
           Reference count:      1
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 20.1.1.1, order 100, rule 3 (active)
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              None

           Referenced by profiles:
              None

           Referenced by merge policies:
              mpl_5

        IP Policy p3
           Administrative state: enable
           Reference count:      1
           Classifier control list: C1, precedence 80
              color yellow
           Classifier control list: C4, precedence 900
              color red

           Referenced by interfaces:
              ATM5/0.1  input policy, statistics disabled, virtual-router default

           Referenced by profiles:
              None

           Referenced by merge policies:
              None

        IP Policy mpl_5
           Administrative state: enable
           Reference count:      1
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)
                   next-hop 20.1.1.1, order 100, rule 3 (reachable)
           Classifier control list: *, precedence 1000
              forward

           Referenced by interfaces:
              ATM5/0.2  output policy, statistics enabled, virtual-router default

           Referenced by profiles:
              None

           Component policies:
              p1
              p2

17. Detach p3 from atm 5/0.1.
    host1(config)#interface atm 5/0.1 host1(config-subif)#no ip policy input p3 host1(config-subif)#exit
18. Detach p1 from atm 5/0.2. Merge policy mpl_5 is detached and deleted and only p2 is now attached.
    host1(config)#interface atm 5/0.2 host1(config-subif)#no ip policy output p1 host1(config-subif)#exit
19. Detach p2 from atm 5/0.2.
    host1(config)#interface atm 5/0.2 host1(config-subif)#no ip policy output p2 host1(config-subif)#exit
20. Display policies to verify that no merge policies exist and that all other policies have a 0 reference count because they are not attached anywhere.

        host1#show policy-list

                                          Policy Table
                                          ------ -----
        IP Policy p1
           Administrative state: enable
           Reference count:      0
           Classifier control list: C2, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 10.1.1.1, order 100, rule 2 (active)

        IP Policy p2
           Administrative state: enable
           Reference count:      0
           Classifier control list: C3, precedence 10
              filter
           Classifier control list: C1, precedence 90
              forward
                 Virtual-router: default
                 List:
                   next-hop 20.1.1.1, order 100, rule 3 (active)
           Classifier control list: *, precedence 1000
              forward

        IP Policy p3
           Administrative state: enable
           Reference count:      0
           Classifier control list: C1, precedence 80
              color yellow
           Classifier control list: C4, precedence 900
              color red

#### Related Topics

- Merging Policies Overview
- Monitoring Policy Management Overview