Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# set metric

#### Syntax

set metric [ +relValue | -relValue | absValue ]

no set metric

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Modifies the metric value (for BGP, the MED) for a route that matches the route map by applying a relative or absolute metric. The no version removes the set clause from a route map.

| Note: You cannot have an absolute and a relative metric within the same route map sequence. Issuing either command overrides any previously configured metric in the route map.

#### Options

- +—Specifies that the value is added to the metric for routes matching the route map; immediately precedes the metric value with no intervening space
- –—Specifies that the value is subtracted from the metric for routes matching the route map; immediately precedes the metric value with no intervening space
- relValue—Number, in the range 0–4294967295
- absValue—Number, in the range 0–4294967295

#### Mode

Route Map Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out