Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- show ipv6 dhcpv6-local binding

# Monitoring DHCPv6 Local Server Binding Information

#### Purpose

Display the mapping between one or more IPv6 addresses and the DHCP unique ID of the subscriber’s computer.

#### Action

To display the DHCP binding information for an IPv6 address:

    host1#show ipv6 dhcpv6-local binding 2001:db8:4::/48

       Prefix           Client DUID        Lease            Intf
    -------------   -------------------   --------   ------------------
    2001:db8:4::/48 <LL 1/00A0DE113502>   infinite   FastEthernet 3/6.1

#### Meaning

Table 1 lists the show ipv6 dhcpv6-local binding command output fields.

Table 1: show ipv6 dhcpv6-local binding Output Fields

Field Name | Field Description
--- | ---
Prefix | IPv6 address
Client DUID | DHCP unique ID of subscriber’s computer
Lease | Time for which the IPv6 address is available in seconds, or infinite
Intf | Router’s interface that is associated with the subscriber’s computer

#### Related Topics

- show ipv6 dhcpv6-local binding

#### Published: 2010-07-20

Help
|
My Account
|
Log Out