Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# diag-level

#### Syntax

diag-level [ normal ] [ bypass ]

#### Release Information

Command introduced in JunosE Release 9.2.0.

#### Description

Sets the diagnostics level on the active or standby SRP module to reduce boot time during a cold and a warm boot. The default diagnostics level is normal. There is no no version.

#### Options

- normal—executes full diagnostics on the boot of the line card

  bypass—skips diagnostic tests on the boot of the line card

#### Mode

Global Configuration

#### Published: 2010-07-19

Help
|
My Account
|
Log Out