# Monitoring Multiclass MLPPP

#### Purpose

Display information about the status and configuration of multilink classes on an MLPPP Interface.

#### Action

To display configuration information about multiclass MLPPP member links configured in the specified MLPPP bundle:

    host1#show ppp interface mlppp bundle1 config
    PPP interface mlppp mlppp1 is up
    ...

    PPP multilink member-interface gigabitEthernet 3/0.1.1 is up
    Link interface administrative status is open
    PPP multilink multiclass is enabled
    PPP multilink multiclass classes 4
    PPP multilink multiclass fragmentation is enabled on “voice”, otherData”
    PPP multilink multiclass reassembly is enabled on “voice”, ”otherData”
    ...

    PPP multilink member-interface gigabitEthernet 3/0.1.2 is up
    Link interface administrative status is open
    PPP multilink multiclass is enabled
    PPP multilink multiclass classes 4
    PPP multilink multiclass fragmentation is enabled on “voice”,”otherData”
    PPP multilink multiclass reassembly is enabled on “voice”, ”otherData”
    ...
    1 mlppp interfaces found

To display the statistics of the multiclass MLPPP member links configured in the specified MLPPP bundle:

    host1#show ppp interface mlppp bundle1 statistics
    PPP interface mlppp bundle1 is up
    Time since last baseline 2 days, 18 hours
    2 receive classes, 2 transmit classes
    Interface statistics              in                   out
       packets                        0                    0
       octets                         0                    0
       errors                         0                    0
       discards                       0                    0
       fragments                      0                    0

    Receive Class 0:
    0 fragments in reassembly list
    0 reordered, 0/0 discarded fragments/bytes,
    0x0 last received sequence number

    Receive Class 1:
    0 fragments in reassembly list
    0 reordered, 0/0 discarded fragments/bytes,
    0x0 last received sequence number

    Transmit Class 0:
    0 fragments, 0x8 last sent sequence number

    Transmit Class 1:
    0 fragments, 0x0 last sent sequence number
    ...
    1 mlppp interfaces found

To display complete configuration, statistics, and status information of multiclass MLPPP member links configured in the specified MLPPP bundle:

    host1#show ppp interface mlppp bundle1 full
    Bundle name: bundle1
    MLPPP interface gigabitEthernet 3/0.1.1 is up
    Link interface administrative status is open
    PPP multilink multiclass is enabled
    PPP multilink multiclass classes 4
    PPP multilink multiclass fragmentation is enabled on “voice”, otherData”
    PPP multilink multiclass reassembly is enabled on “voice”, ”otherData”
    ...
    LCP negotiated options            local               peer
       max-receive-unit               1590                1590
       max-receive-reconstructed-unit 1590                1590
       authentication                 none                none
       magic-number                   0x78b5606f          0x5aa2de54
       pfc                            none                none
       acfc                           none                none
       multiclass-classes             4			           	    4
       multiclass-sequence-format     long			        	    long
    ...
    1 mlppp interfaces found

#### Meaning

Table 17 lists the show ppp interface mlppp command output fields.

Table 17: show ppp interface mlppp Output Fields

Field Name | Field Description
--- | ---
PPP interface mlppp bundleName | Name and state (up or down) of the MLPPP interface
PPP multilink member-interface interfaceName | Name and state (up or down) of the MLPPP member link interface
Link interface administrative status | Administrative state of the member link interface: open (enabled) or closed (disabled)
PPP multilink multiclass | Configuration of multiclass MLPPP on the MLPPP interface: enabled or disabled
PPP multilink multiclass classes | Number of multilink classes created on the MLPPP interface: 1 through 8
PPP multilink multiclass fragmentation | Configuration of fragmentation of the multiclass MLPPP interface: enabled or disabled. If fragmentation is enabled then the command also lists the QoS traffic classes on which fragmentation is enabled.
PPP multilink multiclass reassembly | Configuration of reassembly of the multiclass MLPPP interface: enabled or disabled. If reassembly is enabled then it also lists the QoS traffic classes on which reassembly is enabled.
mlppp interfaces found | Number of MLPPP interfaces configured
Time since last baseline | When baselining is configured, the time since the last baseline was set is displayed in hours:minutes:seconds or days/hours format
receive class, transmit class | Number of multilink classes configured on the MLPPP bundle
Interface statistics | Statistics for data received by (in) and transmitted (out) on the MLPPP interface: packets—Number of packets received and transmitted on the interface octets—Number of octets received and transmitted on the interface errors—Number of errors received and transmitted on the interface discards—Number of packets discarded on receipt or discarded before they were transmitted fragments—Number of fragments received and transmitted on the interface
Receive Class number | Information about the packets of the specified multilink class received by the router
fragments in reassembly list | Number of buffered fragments reassembled
reordered | Number of fragments reordered
discarded fragments/bytes | Number of fragments and bytes that have been discarded.
last received sequence number | Sequence number of the last multiclass MLPPP packet received
Transmit Class number | Information about the packets of the specified multilink class transmitted by the router
fragments | Number of fragments that are sent by the router
last sent sequence number | Sequence number of the last multiclass MLPPP packet sent
Bundle name | Name of the MLPPP bundle
MLPPP interface interfaceName | Name and state (up or down) of the configured MLPPP interface
LCP negotiated options | Negotiated LCP options for the local and peer systems: max-receive-unit—Negotiated maximum receive unit, in octets, for the local and remote (peer) side of the link max-receive-reconstructed-unit—Negotiated maximum receive reconstructed unit, in octets, for the local and remote (peer) side of the link authentication—Negotiated authentication method (none, pap, or chap) for the local and remote (peer) side of the link magic-number—Negotiated magic number for the local and remote (peer) side of the link pfc—Negotiated protocol field compression (none or enabled) for the local and remote (peer) side of the link acfc—Negotiated address and control field compression (none or enabled) for the local and remote (peer) side of the link multiclass-classes—Number of multilink classes negotiated multiclass-sequence-format—Format of the negotiated sequence number: long or short

#### Related Topics

- Configuring Multiclass MLPPP
- show ppp interface