Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Enabling Multiclass MLPPP
- Configuring Multiclass MLPPP

# ppp multilink multiclass

#### Syntax

ppp multilink multiclass [ multilink-classes classNumber ]

no ppp multilink multiclass [ multilink-classes ]

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Enables multiclass MLPPP on the router, and optionally creates a specified number of multilink classes. The no version without the multilink-classes keyword disables multiclass MLPPP on the router. The no version with the multilink-classes keyword restores the number of multilink classes to the default value, 1.

#### Options

- classNumber—Number of multilink classes that can be created in the range 1–8, with a default value of 1.

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

#### Related Topics

- Enabling Multiclass MLPPP
- Configuring Multiclass MLPPP

#### Published: 2010-07-13

Help
|
My Account
|
Log Out