Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# sscc protocol lac

#### Syntax

[ no ] sscc protocol lac

#### Release Information

Command introduced in JunosE Release 11.0.0.

#### Description

Configures the SRC client to support policy and QoS configuration on L2TP interfaces on a virtual router that functions as an L2TP access concentrator (LAC) on one side of an L2TP tunnel. The no version disables SRC client support for L2TP LAC interfaces.

| Note: You must enable the SRC client by using the sscc enable cops-pr command on the virtual router to be able to configure policy and QoS support for L2TP LAC interfaces by the COPS messages.

#### Mode

Global Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out