[ Contents] [ Prev] [ Next] [ Report an Error]

# HSSI Module Combination

> Line module label | HSSI-3F
> I/O module label | HSSI-3 I/O
> Number of I/O ports | 3
> Software release | First supported: 3.1.0 Final supported: 7.3.x
> Description | 60 W High-speed serial interface
> Type | Non-ASIC
> Capability | Up to 44.736 MHz data rate HDLC Framing
> Software features | See ERX Module Guide, Appendix A, Module Protocol Support for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | ERX-7xx models ERX-1410 router
> SRP module compatibility | SRP-5G SRP-5G+ SRP-10G
> Module redundancy support | Not applicable
> Cables and connectors | Standard HSSI connector: 2-row, 50-pin, receptacle header with rails and latch blocks 50 feet (15.24 m) maximum cable length See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See ERX Module Guide, Appendix B, Module LEDs.
> Alarms, errors, and events | See Monitoring Interfaces in the Configuring HSSIs chapter of the JUNOSe Physical Layer Configuration Guide for Release 8.0.x and earlier.

[ Contents] [ Prev] [ Next] [ Report an Error]