# encapsulation frame-relay ietf

#### Syntax

encapsulation frame-relay ietf

no encapsulation frame-relay

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables Frame Relay encapsulation. The no version removes Frame Relay configuration from an interface.

#### Mode

Interface Configuration

#### Related Topics

- Configuring Frame Relay Layer 2 Services in the JunosE BGP and MPLS Configuration Guide