Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# ip pim dr-priority

#### Syntax

ip pim dr-priority priority

no ip pim dr-priority

#### Release Information

Command introduced in JunosE Release 9.0.0.

Router Configuration mode added in JunosE Release 10.0.0.

#### Description

Assigns a priority for the interface to be selected as the designated router. An interface with a higher priority value is preferred as a designated router over an interface with a lower priority value. In Interface Configuration mode, the no version restores the value that is specified in Router Configuration mode. If the designated router priority is not specified in Router Configuration mode, then the default value of 1 is restored.

| Note: You cannot configure the designated router priority on PIM dense mode interfaces.

#### Options

- priority—Value in the range 1–254; default value is 1.

#### Mode

Interface Configuration, Router Configuration

#### Published: 2010-07-19

Help
|
My Account
|
Log Out