Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Creating a Two-Rate Rate-Limit Profile

# peak-burst

#### Syntax

peak-burst size { millisecond milliseconds }

no peak-burst

#### Release Information

Command introduced before JunosE Release 7.1.0.
milliseconds variable added in JunosE Release 8.1.0.

#### Description

Sets the peak burst for a rate-limit profile. The no version restores the default value, 100 ms; if 100ms is less than 8K, then 8K (8192).

#### Options

- size—Size in bytes in the range 1–4294967295
- milliseconds—Milliseconds in the range 1–10000

#### Mode

Rate Limit Profile Configuration

#### Related Topics

- Creating a Two-Rate Rate-Limit Profile

#### Published: 2010-07-13

Help
|
My Account
|
Log Out