Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# debounce

#### Syntax

debounce [ seconds ]

no debounce

#### Release Information

Command introduced in JunosE Release 9.3.0.

#### Description

Enables the debounce timer and sets the time interval that the interface waits before reporting a state change to the upper-layer protocols. The no version restores the default behavior, disabling debounce on the interface.

#### Options

- seconds—Interval for which an interface must maintain a given state before the interface reports the state change to the upper-layer protocols. Number in the range 1–5 seconds; default value is 1 second.

#### Mode

Interface Configuration

#### Published: 2010-07-19

Help
|
My Account
|
Log Out