Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# remote-neighbor

#### Syntax

For OSPF:

[ no ] remote-neighbor ipAddress area { areaId | areaIdInt }

For PIM:

[ no ] remote-neighbor [ ipAddress | ipv6Address ] sparse-mode

For RIP:

[ no ] remote-neighbor ipAddress

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an OSPF, PIM, or RIP remote neighbor. The no version removes the remote neighbor and any attributes configured for the neighbor.

| Note: For PIM, this command is typically used when you configure PIM remote neighbors to run multicast services over BGP/MPLS VPNs. That functionality is no longer supported.

#### Options

- ipAddress—IPv4 address identifying the remote neighbor
- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value, in the range 0–4294967295
- ipv6Address—IPv6 address identifying the remote neighbor

#### Mode

Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out