Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Attaching a QoS Profile to an Interface

# svlan qos-profile

#### Syntax

[ no ] svlan s-vlanIdValue qos-profile qosProfileName

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Attaches a QoS profile to the specified S-VLAN ID on the interface. The no version detaches the QoS profile from the S-VLAN ID.

#### Options

- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- qosProfileName—Name of the QoS profile that you want to attach to the S-VLAN ID

#### Mode

Interface Configuration

## Related Documentation

- Attaching a QoS Profile to an Interface

#### Published: 2010-10-19

Help
|
My Account
|
Log Out