# Monitoring Dial-out Targets within the Current VR Context

#### Purpose

Display configured dial-out targets within the current virtual router context.

This command displays aspects of the dial-out state machine and details about the dial-out routes themselves. This section presents sample output. The actual output on your router may differ significantly.

#### Action

To display general information for all targets within the virtual router:

    host1:dialout#show l2tp dial-out target
    Target         Status     Active Sessions
    ------         ------     --------------
    10.10.1.1/16   up         14
    10.1.1.0/24    up         10

To display detailed information about a particular target, specify the target IP address and mask:

    host1:dialout#show l2tp dial-out target 10.1.1.0/24
    Target 10.1.1.0/24
    Operational status: up
    Active sessions: 10
    Total triggers: 127
    Failed sessions: 2
    Connected sessions: 8

To display aggregate counts for targets in each of the possible operational and administrative states:

    host1:dialout#show l2tp dial-out target summary

To display detailed configuration, state, and statistics:

    host1:dialout#show l2tp dial-out target detail

To display information about the operational or administrative state:

    host1:dialout#show l2tp dial-out target state inService

To displays dial-out information across all virtual routers:

    host1:dialout#show l2tp dial-out target allVirtualRouters

| Note: The level of a user’s permission determines the use of the allVirtualRouters option. For example, if you have permission to view only the current virtual router, then that is all that is displayed when you enter a command.

#### Meaning

Table 96 lists the show l2tp dial-out target command output fields.

Table 96: show l2tp dial-out target Output Fields

Field Name | Field Description
--- | ---
Target | Address of the target
Status | Status of the connection to the target
Active Sessions | Currently active session to the target
Total triggers | Trigger packets received for the target
Failed sessions | Sessions that are currently in the failed state
Connected sessions | Sessions that are currently in the connected state

#### Related Documentation

- For detailed information about operational states, see Dial-Out Operational States
- show l2tp dial-out target