Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# tunnel mpls autoroute announce

#### Syntax

[ no ] tunnel mpls [ traffic-eng ] autoroute announce [ ospf | isis ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the LSP tunnel to register its endpoint (the egress router) with the configured routing protocol so that the protocol can use the tunnel to determine routes. If you do not specify a routing protocol, the default is both IS-IS and OSPF. The no version disables endpoint announcements.

#### Options

- traffic-eng—Specifies optional keyword for compatibility with non–E Series implementations
- ospf—Endpoint is announced to OSPF
- isis—Endpoint is announced to IS-IS

#### Mode

Interface Configuration, Tunnel Profile Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out