# Monitoring the Configuration of the RADIUS Relay Server

#### Purpose

Display information about the RADIUS relay server configuration.

#### Action

To display the RADIUS relay server configuration:

    host1#show radius relay servers

    RADIUS Relay Authentication Server Configuration
    ------------------------------------------------
     IP Address         IP Mask        Secret
    -------------   ---------------   ---------
    10.10.8.15      255.255.255.255   newsecret
    192.168.102.5   255.255.255.255   999Y2K
    Udp Port: 1812

    RADIUS Relay Accounting Server Configuration
    --------------------------------------------
     IP Address         IP Mask       Secret
    -------------   ---------------   -------
    10.10.1.0       255.255.255.0     NO8pxq
    192.168.102.5   255.255.255.255   12BE$56
    Udp Port: 1813

#### Meaning

Table 62 lists the show radius relay servers command output fields.

Table 62: show radius relay servers Output Fields

Field Name | Field Description
--- | ---
IP Address | Address of the RADIUS relay server
IP Mask | Mask of the RADIUS relay server
Secret | Secret used for exchanges between the RADIUS relay server and client
Udp Port | Router’s port on which the RADIUS relay server listens

#### Related Documentation

- show radius relay servers