# Example: Commonly Used VRRP Configuration

Figure 7 shows two physical routers backing up each other through VRRP. Routers R1 and R2 are both configured with VRID 1 and VRID 2. In this configuration, under normal circumstances the routing load is distributed between the two routers.

Figure 7: Commonly Used VRRP Configuration

#### Related Documentation

- VRRP Overview
- VRRP Implementation in E Series Routers
- VRRP Router Election Rules
- Before You Configure VRRP
- Configuring VRRP