Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring the Scheduler Hierarchy for Hashed Load Balancing in 802.3ad Link Aggregation Groups
- Configuring the Scheduler Hierarchy for Subscriber Load Balancing in 802.3ad Link Aggregation Groups
- Creating Parameter Instances
- For more information about other fields displayed with this command, see the JunosE Physical Layer Configuration Guide
- show interfaces lag members

# Monitoring the QoS Configuration of IEEE 802.3ad Link Aggregation Group Bundles

#### Purpose

Display information about the QoS configuration for Ethernet member links in all IEEE 802.3ad link aggregation group (LAG) bundles configured on the router, or about the member links in a specified IEEE 802.3ad LAG bundle.

#### Action

To display the QoS configuration for a specific LAG bundle:

    host1#show interfaces lag lg0 members
    Lag lg0 is Up, Administrative status is Up
    MAC Address is 0090.1a40.01be
    MTU: Operational 1526
    Duplex Mode: Operational Full Duplex
    Speed: Operational 100 Mbps
    System Priority 32768 System MAC Address is 0090.1a00.00e0 key 8
    Partner System Priority 0 System MAC Address is 0000.0000.0000 key 0
    QoS parameter: vlan 1500000
    Attached QoS profile: eth1
    Member-interface FastEthernet11/2 is Up
    (LACP disabled, state collecting/distributing)
    Member-interface FastEthernet11/3 is Down
    (LACP disabled, state waiting)
    Member-interface FastEthernet11/4 is Up
    (LACP disabled, state collecting/distributing)

#### Meaning

Table 1 lists the related show interfaces lag memberscommand output fields.

Table 1: show interfaces lag members Output Fields

Field Name | Field Description
--- | ---
Lag | Name of the LAG bundle
QoS parameter | QoS parameter instance at the displayed interface
Attached QoS profile | QoS profile attachment at the displayed interface

## Related Documentation

- Configuring the Scheduler Hierarchy for Hashed Load Balancing in 802.3ad Link Aggregation Groups
- Configuring the Scheduler Hierarchy for Subscriber Load Balancing in 802.3ad Link Aggregation Groups
- Creating Parameter Instances
- For more information about other fields displayed with this command, see the JunosE Physical Layer Configuration Guide
- show interfaces lag members

#### Published: 2010-10-04

Help
|
My Account
|
Log Out