# show ip bgp next-hops

#### Syntax

show ip bgp [ ipv4 unicast | ipv4 multicast | vpnv4 all | vpnv4 vrf vrfName |
l2vpn all | l2vpn vpls vplsName | l2vpn vpws vpwsName } | route-target signaling ]
next-hops [ ipAddress ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
l2vpn and all keywords added in JunosE Release 7.1.0.
vpls keyword and vplsName variable added in JunosE Release 7.1.0.
vpws keyword and vpwsName variable added in JunosE Release 8.1.0.
route-target signaling keywords added in JunosE Release 8.2.0.

#### Description

Displays information about BGP next hops.

#### Options

- ipv4 unicast—Specifies the IPv4 unicast address family and routing table; the default option
- ipv4 multicast—Specifies the IPv4 multicast address family and routing table
- vpnv4 all—Specifies the IPv4 VPN address family and all IPv4 VPN routing and forwarding instances
- vpvn4 vrf vrfName—Specifies the IPv4 VPN address family and only the IPv4 VPN routing and forwarding instance with the name vrfName
- l2vpn all—Specifies all VPLS and VPWS instances in the L2VPN address family
- l2vpn vpls vplsName—Specifies the VPLS instance with the name vplsName
- l2vpn vpws vpwsName—Specifies the VPWS instance with the name vpwsName
- route-target signaling—Displays information for only the route-target address family
- ipAddress—Displays information only for this indirect next hop
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Documentation

- Monitoring BGP-Related Settings for L2VPNs, Monitoring BGP Next Hops for L2VPNs, and Monitoring BGP Next Hops for VPLS in the JunosE BGP and MPLS Configuration Guide