Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# timeout

#### Syntax

RADIUS:

timeout waitTime

no timeout

RTR:

timeout timeoutValue

no timeout

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

When used from RADIUS Configuration mode, specifies the interval, in seconds, before the router retransmits a RADIUS packet to an authentication or accounting server. The no version restores the default.

When used from RTR Configuration mode, specifies the timeout for a Response Time Reporter operation. The no version returns the operation to the default value. You can apply this parameter only to echo entries.

#### Options

- waitTime—Number of seconds in the range 1–1000; default value is 3
- timeoutValue—Number in milliseconds that the operation waits for a response; if the value is set to 0 or is larger than frequency, it will be ignored; default value is 5000

#### Mode

RADIUS Configuration, RTR Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out