Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring S-VLAN Tunnels for Layer 2 Services in the JunosE BGP and MPLS Configuration Guide

# svlan ethertype

#### Syntax

svlan ethertype ethertypeValue

no svlan ethertype

#### Release Information

Command introduced before JunosE Release 7.1.0.
88a8 keyword added in JunosE Release 7.1.0.

#### Description

In Interface Configuration mode, specifies the Ethertype of an S-VLAN. The no version restores the default value, 9100.

In Profile Configuration mode, specifies the available Ethertypes that the packet must use to create a dynamic VLAN subinterface. The no version restores the default value, autoconfig.

#### Options

- ethertypeValue—One of the following Ethertype values:
  - 8100—Specifies Ethertype value 0x8100, as defined in IEEE Standard 802.1q
  - 88a8—Specifies Ethertype value 0x88a8, as defined in draft IEEE Standard 802.1ad
  - 9100—Specifies Ethertype value 0x9100, which is the default for Interface Configuration mode
  - autoconfig—Specifies in a VLAN profile that the packet can use any Ethertype to create a dynamic VLAN subinterface; this is the default for Profile Configuration mode

#### Mode

Interface Configuration, Profile Configuration

## Related Documentation

- Configuring S-VLAN Tunnels for Layer 2 Services in the JunosE BGP and MPLS Configuration Guide

#### Published: 2010-10-19

Help
|
My Account
|
Log Out