Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# table-map

#### Syntax

table-map mapTag

For removing route maps for IS-IS IPv6 only:

no table-map

For removing route maps for all other cases:

no table-map [ mapTag ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Applies the specified route map to all BGP, IS-IS, OSPF, or RIP routes about to be added to the IP routing table. The no version halts application of the route map.

#### Options

- mapTag—A string of up to 32 alphanumeric characters that specifies the name of the route map; for each protocol, the route map can set only the following values:
  - BGP—Distance, IP next hop, level, metric, metric type, route type, and tag values
  - IS-IS—Distance, level, metric, metric type, origin, preference, route type, and tag values; IS-IS IPv6 supports only a single route map
  - OSPF—Distance, metric, metric type, route type, and tag values
  - RIP—Distance, metric, and tag values

#### Mode

Address Family Configuration (BGP, IS-IS, RIP), Router Configuration (BGP, IS-IS, OSPF, RIP)

#### Published: 2010-10-19

Help
|
My Account
|
Log Out