Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# priority burst

#### Syntax

priority priorityValue burst burstSize

no priority priorityValue burst

#### Release Information

Command introduced in JunosE Release 8.1.0.

#### Description

Sets the burst size for each priority. The no version returns to the default value.

#### Options

- priorityValue–Hi-Green-IC, Hi-Green-SC, Hi-Yellow-IC, Hi-Yellow-SC, Lo-Green-IC, Lo-Green-SC, Lo-Yellow-IC, Lo-Yellow-SC
- burstSize—Number of packets, in the range 32–65535; 0 denotes no burst size: default value is equal to half of the configured maximum rate

#### Mode

DoS Protection Group Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out