Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Policy Rule Precedence
- Creating a One-Rate Rate-Limit Profile
- Creating a Two-Rate Rate-Limit Profile

# rate-limit-profile

#### Syntax

To create or modify a rate-limit profile:

[ no ] profileType rate-limit-profile profileName [ rateLimitType ]

To specify a rate-limit profile in a policy in classifier-group mode:

[ no ] [ suspend ] rate-limit-profile profileName

To create a hierarchical rate-limit profile:

[ no ] rate-limit-profile profileName [ two-rate | one-rate ] hierarchical

To specify a rate-limit for an external parent group:

rate-limit-profile profileName

no rate-limit-profile

#### Release Information

Command introduced before JunosE Release 7.1.0.
hierarchical keyword added in JunosE Release 7.2.0.
Parent Group Configuration mode added in JunosE Release 8.0.0.

#### Description

From Global Configuration mode, creates a rate-limit profile and enters Rate Limit Profile Configuration mode. The no version deletes the rate-limit profile.

From Classifier Group Configuration mode, creates a rate-limit profile rule in a policy list. The no version removes a rate-limit profile from a policy list; the suspend version suspends the rule; the no suspend resumes a suspended rule.

| Note: The Classifier Group Configuration mode version of the rate-limit-profile command replaces the Policy List Configuration mode version, which may be removed completely in a future release.

From Parent Group Configuration mode, creates a parent group in a hierarchy.

The hierarchical keyword creates a hierarchical rate limit. The no version removes a hierarchical rate-limit profile.

#### Options

- profileType—ip, ipv6, l2tp, or mpls; for backward compatibility, if you do not specify a profile type, the router creates an IP profile
- profileName—Name of the rate-limit profile
- rateLimitType—One-rate or two-rate

#### Mode

Classifier Group Configuration, Global Configuration, Parent Group Configuration

## Related Documentation

- Policy Rule Precedence
- Creating a One-Rate Rate-Limit Profile
- Creating a Two-Rate Rate-Limit Profile

#### Published: 2010-10-19

Help
|
My Account
|
Log Out