Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# show bgp ipv6 summary

#### Syntax

show bgp ipv6
[ unicast | multicast | vpnv6 all | vpnv6 vrf vrfName | route-target signaling ]
summary [ fields { fieldOptions } ] [ delta ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
route-target signaling keywords added in JunosE Release 8.2.0.

#### Description

Displays filtered information about the status of all BGP connections. Only those fields that you specify are displayed, except that the prefix field is always displayed. Default fields can be set with the default-fields peer command.

#### Options

- unicast—Specifies the IPv6 unicast address family and routing table; the default option
- multicast—Specifies the IPv6 multicast address family and routing table
- vpnv6 all—Specifies the VPN-IPv6 address family and all IPv6 VPN routing and forwarding instances
- vpn6 vrf vrfName—Specifies the VPN-IPv6 address family and only the IPv6 VPN routing and forwarding instance with the name vrfName
- route-target signaling—Displays information for only the route-target address family
- fields—Displays only the specified fields; the display order of the fields is hard-coded and not affected by the order in which you enter them
- fieldOptions—Fields to be displayed, in the format
  all | [ dynamic | intro | last-reset-reason | messages-received | messages-sent | more-in-queue | peer-type | prefixes-received | remote-as | rib-version |
  send-queue-length | state | times-up | up-down-time | updates-received | updates-sent ]*
  - dynamic —Nature of peer, dynamic or not
  - intro—Introductory information about the state of various BGP attributes; this information is displayed only if you specify this keyword
  - last-reset-reason—Reason for most recent reset
  - messages-received—Total number of messages received from the peer
  - messages-sent—Total number of messages sent to the peer
  - more-in-queue—Status indicating whether any messages are waiting to be sent to this peer
  - peer-type—Type of BGP peer: internal, external, or confederation
  - prefixes-received—Number of unique prefixes received from the peer
  - remote-as—Remote AS number of the peer
  - rib-version—Last RIB version queued to be sent to this peer
  - send-queue-length—Number of messages queued to be sent to this peer
  - state—State of the BGP session
  - times-up—Number of times the session has been established
  - up-down-time—How long the session has been up or down
  - updates-received—Number of update messages received from the peer
  - updates-sent—Number of update messages sent to the peer
  - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out