# pppoe url

#### Syntax

pppoe url url

no pppoe url

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Causes the PPPoE application to send a string to the new client. The no version disables the message.

The recipient of the message is determined by the mode from which the command is issued. From Interface Configuration mode the PADM message is sent to the client as it is configured (if connected). From Profile Configuration mode the message is sent to the new client created when the profile is dynamically attached to an IP interface.

#### Options

- url—URL string sent

#### Mode

Interface Configuration, Profile Configuration