Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# nsf t2

#### Syntax

[ no ] nsf t2 { level-1 | level-2 } [ seconds ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the maximum amount of time, in seconds, that an IS-IS restarting router waits for the LSP database to synchronize. You must configure separate instances of the T2 timer for each IS-IS level at which the router operates. The no version restores the default T2 wait time, 30 seconds.

#### Options

- level-1—Sets the T2 wait time independently for level 1 routing
- level-2—Sets the T2 wait time independently for level 2 routing
- seconds—Maximum wait time, in the range 5–120 seconds, for LSP database synchronization; default value is 30 seconds

#### Mode

Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out