Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Monitoring BGP-Related Settings for L2VPNs in the JunosE BGP and MPLS Configuration Guide

# show ip bgp paths

#### Syntax

show ip bgp [ ipv4 unicast | ipv4 multicast | vpnv4 all | vpnv4 vrf vrfName |
l2vpn all | l2vpn vpls vplsName | l2vpn vpws vpwsName | route-target signaling ]
paths [ regularExpression ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
l2vpn and all keywords added in JunosE Release 7.1.0.
vpls keyword and vplsName variable added in JunosE Release 7.1.0.
vpws keyword and vpwsName variable added in JunosE Release 8.1.0.
route-target signaling keywords added in JunosE Release 8.2.0.

#### Description

Displays information about BGP AS paths.

#### Options

- ipv4 unicast—Specifies the IPv4 unicast address family and routing table; the default option
- ipv4 multicast—Specifies the IPv4 multicast address family and routing table
- vpnv4 all—Specifies the IPv4 VPN address family and all IPv4 VPN routing and forwarding instances
- vpvn4 vrf vrfName—Specifies the IPv4 VPN address family and only the IPv4 VPN routing and forwarding instance with the name vrfName
- l2vpn all—Specifies all VPLS and VPWS instances in the L2VPN address family
- l2vpn vpls vplsName—Specifies the VPLS instance with the name vplsName
- l2vpn vpws vpwsName—Specifies the VPWS instance with the name vpwsName
- route-target signaling—Displays information for only the route-target address family
- regularExpression—Regular expression to match that specifies the desired AS paths. See show ip bgp regexp for information about regular expressions.
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring BGP-Related Settings for L2VPNs in the JunosE BGP and MPLS Configuration Guide

#### Published: 2010-10-19

Help
|
My Account
|
Log Out