# source-address

#### Syntax

source-address sourceAddress

no source-address

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies a source IP address for the LAC tunnel endpoint. The no version removes the source address.

#### Options

- sourceAddress—Address of the local tunnel endpoint (the LAC); can be up to 32 characters (no spaces)

#### Mode

Domain Map Tunnel Configuration, Tunnel Group Tunnel Configuration