Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# profile atm1483 bulk-config-name pvc

#### Syntax

profile atm1483 bulk-config-name bulkConfigName pvc vpi vci overrideProfileName

no profile atm1483 bulk-config-name bulkConfigName pvc vpi vci

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Assigns an overriding profile to a single ATM PVC that exists within a VC subrange previously configured with the atm bulk-config command. The profile atm1483 bulk-config-name pvc command enables you to troubleshoot the specified PVC by overriding the currently assigned base profile with one that has debugging attributes enabled. After the overriding profile is assigned, it is used instead of the previously assigned base profile to create any ATM 1483 dynamic subinterface columns over the specified PVC. The no version removes the overriding profile assignment for the PVC and restores the original base profile assignment.

#### Options

- bulkConfigName—Name associated with the VC range configured for use by a dynamic ATM 1483 subinterface, as specified in the atm bulk-config command
- vpi—Virtual path identifier of the PVC; must exist between the starting VPI value and ending VPI value of a bulk-configured VC subrange
- vci—Virtual circuit identifier of the PVC; must exist between the starting VCI value and ending VCI value of a bulk-configured VC subrange
- overrideProfileName—Name of the profile that overrides the previously assigned base profile for the specified ATM PVC

#### Mode

Interface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out