Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# ppp fragmentation

#### Syntax

ppp fragmentation [ fragmentSize ]

no ppp fragmentation

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables fragmentation on an MLPPP link interface and optionally specifies the maximum fragment size, in octets, to be used on the link. The no version disables fragmentation on the link and restores the default fragment size, which is the link’s MTU.

#### Options

- fragmentSize—Maximum allowable size of the fragment, in the range 128–65535; the default fragment size is the link’s MTU

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out